(footprint "Pin_D1.3mm_L10.0mm_W3.5mm_Flat"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "solder Pin_ with flat with hole, hole diameter 1.3mm, length 10.0mm, width 3.5mm, e.g. Ettinger 13.13.865, https://katalog.ettinger.de/#p=434")
	(tags "solder Pin_ with flat fork")
	(property "Reference" "REF**"
		(at 0 2.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Pin_D1.3mm_L10.0mm_W3.5mm_Flat"
		(at 0 -2.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 2.25 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.3mm_L10.0mm_W3.5mm_Flat.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
