(footprint "RJ14_Connfly_DS1133-S4_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "RJ14 connector 6P4C Horizontal http://www.connfly.com/userfiles/image/UpLoadFile/File/2012/10/26/DS1133.pdf")
	(tags "RJ14 connector 6P4C Connfly DS1133")
	(property "Reference" "REF**"
		(at -3.2 -9.64 180)
		(layer "F.SilkS")
	)
	(property "Value" "RJ14_Connfly_DS1133-S4_Horizontal"
		(at 0.81 6.35 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.03 -5.22 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -4.47 -2.3 180)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.53 -2.3 180)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.02 2.54 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.04 0 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.06 2.54 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ14_Connfly_DS1133-S4_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
