(footprint "Wuerth_WR-PHD_610006243021_SMD_2x03_P2.54mm_Vertical"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Connector Wuerth, WR-PHD 2.54mm Dual Socket Header Bottom Entry SMD, Wuerth electronics 610006243021 (https://katalog.we-online.de/em/datasheet/610006243021.pdf), generated with kicad-footprint-generator")
	(tags "Connector Wuerth WR-PHD 2.54mm 610006243021")
	(property "Reference" "REF**"
		(at 0 -5.01 0)
		(layer "F.SilkS")
	)
	(property "Value" "Wuerth_WR-PHD_610006243021_SMD_2x03_P2.54mm_Vertical"
		(at 0 5.21 0)
		(layer "F.Fab")
	)
	(attr smd)
	(pad "1" smd rect
		(at -3.2 -2.54)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -3.2 0)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -3.2 2.54)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at 3.2 -2.54)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at 3.2 0)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at 3.2 2.54)
		(size 1.8 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -2.54)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 0)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 2.54)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -2.54)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 0)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 2.54)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -3.11 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Wuerth.3dshapes/Wuerth_WR-PHD_610006243021_SMD_2x03_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
