(footprint "Converter_DCDC_Murata_MGJ3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Murata MGJ3, 5.2kVDC Isolated 3W Gate Drive, 15V/5V/5V Configurable, 22.61x23.11x14.19mm, https://power.murata.com/datasheet?/data/power/ncl/kdc_mgj3.pdf")
	(tags "DCDC SMD")
	(property "Reference" "REF**"
		(at 0 -12.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Murata_MGJ3"
		(at 0 12.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Copper Keepout"
		(at 0 1.5 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -9.525 -8.89)
		(size 3.38 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -9.525 -3.81)
		(size 3.38 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -9.525 6.35)
		(size 3.38 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -9.525 8.89)
		(size 3.38 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 9.525 8.89)
		(size 3.38 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 9.525 6.35)
		(size 3.38 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 9.525 -8.89)
		(size 3.38 2.16)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 11.305 5.27) (xy 5.295 5.27) (xy 5.295 7.62) (xy -5.295 7.62) (xy -5.295 5.27) (xy -11.305 5.27)
				(xy -11.305 -2.73) (xy 11.305 -2.73)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Murata_MGJ3.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
