(footprint "Converter_DCDC_Murata_NXExSxxxxMC_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Isolated 1W or 2W Single Output SM DC/DC Converters https://www.murata.com/products/productdata/8807031865374/kdc-nxe1.pdf#page=8 https://www.murata.com/products/productdata/8807031898142/kdc-nxe2.pdf#page=9")
	(tags "Isolated 1W or 2W Single Output SM DC/DC Converters")
	(property "Reference" "REF**"
		(at -4 -9.27 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_Murata_NXExSxxxxMC_SMD"
		(at 0 7.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Keepout"
		(at 0.23368 -0.97282 0)
		(layer "Cmts.User")
	)
	(fp_text user "isolation barrier"
		(at -0.01 0.78 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.01016 -2.76606 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.7 -5.08)
		(size 2.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.7 -2.54)
		(size 2.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.7 2.54)
		(size 2.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.7 2.54)
		(size 2.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 4.7 -5.08)
		(size 2.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -6.1 -1.92) (xy 6.1 -1.92) (xy 6.1 1.93) (xy -6.1 1.93)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_Murata_NXExSxxxxMC_SMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
