(footprint "Converter_DCDC_TRACO_TDU1-xxxx_THT"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "DCDC-Converter, TRACO, TDU1-xxxx, 1W, Rev. October 24. 2023 (Script generated with StandardBox.py) (https://www.tracopower.com/products/tdu1.pdf)")
	(tags "DCDC-Converter TRACO TDU1 THT DIP-8 1W")
	(property "Reference" "REF**"
		(at 0.87 -3.57 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_TRACO_TDU1-xxxx_THT"
		(at 3.82 11.47 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.82 3.87 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 7.62)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 7.62 7.62)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 7.62 2.54)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_TRACO_TDU1-xxxx_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
