(footprint "Converter_DCDC_TRACO_TOS06-12SIL_THT"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "DCDC-Converter, TRACO, TOS06-12SIL, 6A, Rev. March 20. 2024 (Script generated with StandardBox.py) (https://www.tracopower.com/products/tos06sil.pdf)")
	(tags "DCDC-Converter POL TRACO TOS06SIL 2.54MM THT SIP-9 6A")
	(property "Reference" "REF**"
		(at -3.15 -2.37 0)
		(layer "F.SilkS")
	)
	(property "Value" "Converter_DCDC_TRACO_TOS06-12SIL_THT"
		(at -2.3 22.87 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -2.3 10.17 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5.08)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 17.78)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 20.32)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_TRACO_TOS06-12SIL_THT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
