(footprint "Crystal_AT310_D3.0mm_L10.0mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Crystal THT AT310 10.0mm-10.5mm length 3.0mm diameter http://www.cinetech.com.tw/upload/2011/04/20110401165201.pdf")
	(tags "['AT310']")
	(property "Reference" "REF**"
		(at -1.75 3 90)
		(layer "F.SilkS")
	)
	(property "Value" "Crystal_AT310_D3.0mm_L10.0mm_Horizontal"
		(at 4.29 3 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.25 8.75 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_AT310_D3.0mm_L10.0mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
