(footprint "D_SMA-SMB_Universal_Handsoldering"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diode, Universal, SMA (DO-214AC) or SMB (DO-214AA), Handsoldering,")
	(tags "Diode Universal SMA (DO-214AC) SMB (DO-214AA) Handsoldering ")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "D_SMA-SMB_Universal_Handsoldering"
		(at 0 3.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -3 0)
		(layer "F.Fab")
	)
	(pad "1" smd trapezoid
		(at -2.9 0)
		(size 3.6 1.7)
		(rect_delta 0.6 0)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd trapezoid
		(at 2.9 0 180)
		(size 3.6 1.7)
		(rect_delta 0.6 0)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMB.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
