(footprint "Littelfuse_PolyZen-LS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf")
	(tags "Diode Polymer Protected Zener Diode Littelfuse LS")
	(property "Reference" "REF**"
		(at 0.58 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Littelfuse_PolyZen-LS"
		(at 1.27 3.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.58 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.72 0)
		(size 0.56 2.21)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.72 -0.635)
		(size 0.56 0.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.72 0.635)
		(size 0.56 0.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/Littelfuse_PolyZen-LS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
