(footprint "Diode_Bridge_DIGITRON_KBPC_T"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Single phase, Bridge rectifier, 28.614x28.614mm, case KBPC_T(FP), https://www.digitroncorp.com/Digitron/media/Files/Datasheets/KBPC15005-SERIES.pdf")
	(tags "diode module")
	(property "Reference" "REF**"
		(at -8.608 -4.3 180)
		(layer "F.SilkS")
	)
	(property "Value" "Diode_Bridge_DIGITRON_KBPC_T"
		(at 9.16675 10.7 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Mounting Drill Hole"
		(at 9.2 5.8 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "(Screw and Washer)"
		(at 9.2 4.6 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "~"
		(at 2.3 14 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "+"
		(at 2.5 -0.025 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "~"
		(at 16.25 0.225 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "-"
		(at 16.2 14 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 9.16675 7.22525 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 9.31 2.96)
		(drill oval 7.31 0.96)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole roundrect
		(at 16.2 -1.75)
		(size 9.31 2.96)
		(drill oval 7.31 0.96)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "3" thru_hole roundrect
		(at 16.2 16.2)
		(size 9.31 2.96)
		(drill oval 7.31 0.96)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "4" thru_hole roundrect
		(at 2.134 16.2)
		(size 9.31 2.96)
		(drill oval 7.31 0.96)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_DIGITRON_KBPC_T.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
