(footprint "Filter_Murata_BNX025"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.murata.com/en-us/products/productdata/8796778004510/QNFH9101.pdf?1496719830000")
	(tags "EMI Filter")
	(property "Reference" "REF**"
		(at -4.4 -5.6 180)
		(layer "F.SilkS")
	)
	(property "Value" "Filter_Murata_BNX025"
		(at -1.9 7.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.75 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.85 -2.1)
		(size 3.8 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 6.85 -2.1)
		(size 3.8 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.85 2.2)
		(size 3.8 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1 5.1)
		(size 7.9 2.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 3.25 -5.1)
		(size 3.4 2.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(pad "4" smd rect
		(at 6.85 2.2)
		(size 3.8 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Murata_BNX025.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
