(footprint "FuseHolder_Blade_ATO_Littelfuse_FLR_178.6165"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Littelfuse fuse holder for ATO/FKS blade fuses, 80V, vertical, 20 x 6mm, PCB thickness up to 1.5mm, http://www.littelfuse.com/~/media/commercial-vehicle/datasheets/automotive-fuse-holders/ato/littelfuse-fuse-holder-ato-flr-pcb-datasheet.pdf")
	(tags "ATO FKS blade fuse holder")
	(property "Reference" "REF**"
		(at 6.4 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "FuseHolder_Blade_ATO_Littelfuse_FLR_178.6165"
		(at 6.4 5.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 6.4 1.25 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 6.4 1.25)
		(size 2.4 2.4)
		(drill 2.4)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 2.5)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 3.5 0)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 3.5 2.5)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 9.3 0)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 9.3 2.5)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 12.8 0)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 12.8 2.5)
		(size 2.2 2.2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/FuseHolder_Blade_ATO_Littelfuse_FLR_178.6165.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
