(footprint "Fuse_Blade_ATO_directSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "car blade fuse direct solder")
	(tags "car blade fuse")
	(property "Reference" "REF**"
		(at 4.65 -3.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuse_Blade_ATO_directSolder"
		(at 4.6 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.75 -1.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 8 3.8)
		(drill oval 6 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 9.3 0)
		(size 8 3.8)
		(drill oval 6 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Blade_ATO_directSolder.wrl"
		(offset
			(xyz 4.571999931 0 0)
		)
		(scale
			(xyz 0.39 0.39 0.39)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
