(footprint "Fuse_Littelfuse-NANO2-885"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Littelfuse NANO2, 350VAC, 450/500VDC, 10.86 x 4.78 x 4.78mm, https://www.littelfuse.com/media?resourcetype=datasheets&itemid=888f12ed-ed3b-4b45-b910-06af8854ad76&filename=littelfuse-fuse-885-datasheet")
	(tags "Fuse Nano2 885")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Fuse_Littelfuse-NANO2-885"
		(at 0 3.2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -5.275 0)
		(size 5.625 7.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.04464285714)
	)
	(pad "2" smd roundrect
		(at 5.275 0)
		(size 5.625 7.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.04464285714)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-885.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
