(footprint "Fuseholder_Keystone_3555-2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Maxi APX ATX Automotive Blade Fuse Clip Holder https://www.keyelco.com/userAssets/file/M65p40.pdf")
	(tags "Maxi APX ATX Automotive Blade Fuse Clip Holder")
	(property "Reference" "REF**"
		(at 14.75 4.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fuseholder_Keystone_3555-2"
		(at 14.75 -4.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 14.75 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 90)
		(size 6 6)
		(drill 3.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.4)
	)
	(pad "1" thru_hole roundrect
		(at 8.4 0)
		(size 6 6)
		(drill 3.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.4)
	)
	(pad "2" thru_hole circle
		(at 21.1 0)
		(size 6 6)
		(drill 3.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 29.5 0)
		(size 6 6)
		(drill 3.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Keystone_3555-2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
