(footprint "Heatsink_38x38mm_SpringFixation"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Heatsink, 38x38mm, Spring Fixation, diagonal,")
	(tags "heatsink")
	(property "Reference" "REF**"
		(at 20.32 -30.988 0)
		(layer "F.SilkS")
	)
	(property "Value" "Heatsink_38x38mm_SpringFixation"
		(at 17.272 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 19.05 -19.05 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -5.588 -52.832)
		(size 2.99974 2.99974)
		(drill 1.09982)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -5.588 -47.244)
		(size 2.99974 2.99974)
		(drill 1.09982)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 43.688 9.144)
		(size 2.99974 2.99974)
		(drill 1.09982)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 43.688 14.732)
		(size 2.99974 2.99974)
		(drill 1.09982)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Heatsink.3dshapes/Heatsink_38x38mm_SpringFixation.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
