(footprint "L_Bourns_SRP1038C_10.0x10.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Bourns SRP1038C series SMD inductor http://www.bourns.com/docs/Product-Datasheets/SRP1038C.pdf")
	(tags "Bourns SRP1038C SMD inductor")
	(property "Reference" "REF**"
		(at 0.1 -6.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Bourns_SRP1038C_10.0x10.0mm"
		(at 0 6.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.475 0)
		(size 3.55 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 4.475 0)
		(size 3.55 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRP1038C_10.0x10.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
