(footprint "L_Coilcraft_1515SQ-68N"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, Coilcraft, 1515SQ-68N, 5.33x3.56x3.73mm, (https://www.coilcraft.com/getmedia/a4eed406-a97e-4630-9d8e-771bb470867f/1515sq.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor sq")
	(property "Value" "L_Coilcraft_1515SQ-68N"
		(at 0 3.225 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -3.225 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.415 0)
		(size 1.78 4.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.140449)
	)
	(pad "2" smd roundrect
		(at 2.415 0)
		(size 1.78 4.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.140449)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_1515SQ-68N.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
