(footprint "L_Coilcraft_2222SQ-161"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, Coilcraft, 2222SQ-161, 7.37x5.59x5.69mm, (https://www.coilcraft.com/getmedia/a4eed406-a97e-4630-9d8e-771bb470867f/1515sq.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor sq")
	(property "Value" "L_Coilcraft_2222SQ-161"
		(at 0 4.365 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -4.365 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.3 0)
		(size 2.16 6.73)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.115741)
	)
	(pad "2" smd roundrect
		(at 3.3 0)
		(size 2.16 6.73)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.115741)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_2222SQ-161.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
