(footprint "L_Coilcraft_MSS1514V-XXX"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Inductor, Coilcraft, MSS1514V-XXX, 15.0x15.0x8.6mm, (https://www.coilcraft.com/getmedia/a1319e1c-d611-4bc0-be30-c17e52e4e667/mss1514v.pdf), generated with kicad-footprint-generator gen_inductor.py")
	(tags "Inductor mss")
	(property "Value" "L_Coilcraft_MSS1514V-XXX"
		(at 0 8.5 0)
		(layer "F.Fab")
	)
	(property "Reference" "REF**"
		(at 0 -8.5 0)
		(layer "F.SilkS")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -5.75 0)
		(size 3.8 6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.065789)
	)
	(pad "2" smd roundrect
		(at 5.75 0)
		(size 3.8 6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.065789)
	)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_MSS1514V-XXX.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
