(footprint "L_Wuerth_WE-TPC-3816"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "L_Wuerth_WE-TPC-3816 StepUp generated footprint, http://katalog.we-online.de/pbs/datasheet/7440310047.pdf")
	(tags "wurth wuerth smd inductor")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Wuerth_WE-TPC-3816"
		(at 0 3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at 0 -1.75)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 2.15 1.2) (xy 1.177922 1.2) (xy 1.064578 1.003895) (xy 0.918917 0.830439) (xy 0.745359 0.684899)
					(xy 0.549174 0.571693) (xy 0.336318 0.494257) (xy 0.113252 0.454942) (xy -0.113252 0.454942) (xy -0.336318 0.494257)
					(xy -0.549174 0.571693) (xy -0.745359 0.684899) (xy -0.918917 0.830439) (xy -1.064578 1.003895)
					(xy -1.177922 1.2) (xy -2.15 1.2) (xy -2.15 -0.4) (xy 2.15 -0.4)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 0 1.75)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -1.064578 -1.003895) (xy -0.918917 -0.830439) (xy -0.745359 -0.684899) (xy -0.549174 -0.571693)
					(xy -0.336318 -0.494257) (xy -0.113252 -0.454942) (xy 0.113252 -0.454942) (xy 0.336318 -0.494257)
					(xy 0.549174 -0.571693) (xy 0.745359 -0.684899) (xy 0.918917 -0.830439) (xy 1.064578 -1.003895)
					(xy 1.177922 -1.2) (xy 2.15 -1.2) (xy 2.15 0.4) (xy -2.15 0.4) (xy -2.15 -1.2) (xy -1.177922 -1.2)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Wuerth_WE-TPC-3816.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
