(footprint "L_Wuerth_WE-XHMI-8080"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Wuerth, WE-XHMI 8080, 8.3mmx8.8mm (Script generated with StandardBox.py) (https://www.we-online.com/components/products/datasheet/74439358068.pdf)")
	(tags "Inductor Wuerth WE-XHMI 8080")
	(property "Reference" "REF**"
		(at -1.65 -5.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Wuerth_WE-XHMI-8080"
		(at 0 5.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.5 0)
		(size 1.6 7.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 2.5 0)
		(size 1.6 7.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Wuerth_WE-XHMI-8080.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
