(footprint "L_CommonMode_TDK_B82767S4263N030"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "26A , 3Phase N, Quadruple Coil,  https://www.tdk-electronics.tdk.com/inf/30/ds/b82767s4.pdf")
	(tags "common mode filter quadruple choke")
	(property "Reference" "REF**"
		(at -11.936466 -0.598146 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonMode_TDK_B82767S4263N030"
		(at 9.063534 56.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 9.063534 24.901854 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 20)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at -15.83832 33.965388 20)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 18.127068 49.803708 20)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 33.965388 15.83832 20)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 2.159748 21.971371 357)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 6.133051 31.80564 357)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 15.96732 27.832337 357)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 11.994017 17.998068 357)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_CommonMode_TDK_B82767S4263N030.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
