(footprint "L_Mount_Lodestone_VTM254"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Lodestone Pacific, 64.51mm diameter vertical toroid mount, 16AWG/1.27mm holes, https://www.lodestonepacific.com/wp-content/uploads/2020/07/VTM-Series-Full-Page.pdf")
	(tags "vertical inductor toroid mount")
	(property "Reference" "REF**"
		(at 15.24 -21.19 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Mount_Lodestone_VTM254"
		(at 15.24 3.41 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 15.24 -8.89 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 30.48 -17.78)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -17.78)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 30.48 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Mount_Lodestone_VTM254.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
