(footprint "L_Radial_D10.5mm_P4.00x5.00mm_Murata_1200RS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Radial, Pitch=4.00x5.00mm, Diameter=10.5mm, Murata 1200RS, http://www.murata-ps.com/data/magnetics/kmp_1200rs.pdf")
	(tags "Inductor Radial Murata 1200RS")
	(property "Reference" "REF**"
		(at 2 -4.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Radial_D10.5mm_P4.00x5.00mm_Murata_1200RS"
		(at 2 9.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2 2.5 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at 0 5)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 4 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 4 5)
		(size 2.6 2.6)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D10.5mm_P4.00x5.00mm_Murata_1200RS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
