(footprint "L_Radial_D14.2mm_P10.00mm_Neosid_SD14"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Radial series, Radial, pin pitch=10.00mm, , diameter=14.2mm, Neosid, SD14, http://www.neosid.de/produktblaetter/neosid_Festinduktivitaet_Sd14.pdf")
	(tags "Inductor Radial series Radial pin pitch 10.00mm  diameter 14.2mm Neosid SD14")
	(property "Reference" "REF**"
		(at 5 -8.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Radial_D14.2mm_P10.00mm_Neosid_SD14"
		(at 5 8.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10 0)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D14.2mm_P10.00mm_Neosid_SD14.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
