(footprint "L_Radial_D24.4mm_P23.40mm_Murata_1400series"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Radial series, Radial, pin pitch=23.40mm, , diameter=24.4mm, muRATA, 1400series, http://www.murata-ps.com/data/magnetics/kmp_1400.pdf")
	(tags "Inductor Radial series Radial pin pitch 23.40mm  diameter 24.4mm muRATA 1400series")
	(property "Reference" "REF**"
		(at 11.7 -13.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Radial_D24.4mm_P23.40mm_Murata_1400series"
		(at 11.7 13.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.7 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 23.4 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D24.4mm_P23.40mm_Murata_1400series.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
