(footprint "L_Radial_D7.0mm_P3.00mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Radial series, Radial, pin pitch=3.00mm, , diameter=7mm, http://www.abracon.com/Magnetics/radial/AIUR-16.pdf")
	(tags "Inductor Radial series Radial pin pitch 3.00mm  diameter 7mm")
	(property "Reference" "REF**"
		(at 1.5 -4.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Radial_D7.0mm_P3.00mm"
		(at 1.5 4.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.5 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D7.0mm_P3.00mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
