(footprint "L_Radial_L10.2mm_W10.2mm_Px7.62mm_Py7.62mm_Pulse_LP-30"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Radial series, Radial, pin pitch=7.62*7.62mm^2, , length*width=10.16*10.16mm^2, Pulse, LP-30, http://datasheet.octopart.com/PE-54044NL-Pulse-datasheet-5313493.pdf")
	(tags "Inductor Radial series Radial pin pitch 7.62*7.62mm^2  length 10.16mm width 10.16mm Pulse LP-30")
	(property "Reference" "REF**"
		(at 3.81 -10.14 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Radial_L10.2mm_W10.2mm_Px7.62mm_Py7.62mm_Pulse_LP-30"
		(at 3.81 2.52 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.81 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.62 -7.62)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_L10.2mm_W10.2mm_Px7.62mm_Py7.62mm_Pulse_LP-30.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
