(footprint "L_Radial_L12.6mm_W12.6mm_Px9.52mm_Py9.52mm_Pulse_LP-37"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Radial series, Radial, pin pitch=9.52*9.52mm^2, , length*width=12.57*12.57mm^2, Pulse, LP-37, http://datasheet.octopart.com/PE-54044NL-Pulse-datasheet-5313493.pdf")
	(tags "Inductor Radial series Radial pin pitch 9.52*9.52mm^2  length 12.57mm width 12.57mm Pulse LP-37")
	(property "Reference" "REF**"
		(at 4.76 -12.295 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Radial_L12.6mm_W12.6mm_Px9.52mm_Py9.52mm_Pulse_LP-37"
		(at 4.76 2.775 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.76 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 9.52 -9.52)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_L12.6mm_W12.6mm_Px9.52mm_Py9.52mm_Pulse_LP-37.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
