(footprint "L_Radial_L9.1mm_W9.1mm_Px6.35mm_Py6.35mm_Pulse_LP-25"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Radial series, Radial, pin pitch=6.35*6.35mm^2, , length*width=9.14*9.14mm^2, Pulse, LP-25, http://datasheet.octopart.com/PE-54044NL-Pulse-datasheet-5313493.pdf")
	(tags "Inductor Radial series Radial pin pitch 6.35*6.35mm^2  length 9.14mm width 9.14mm Pulse LP-25")
	(property "Reference" "REF**"
		(at 3.175 -8.995 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Radial_L9.1mm_W9.1mm_Px6.35mm_Py6.35mm_Pulse_LP-25"
		(at 3.175 2.645 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.175 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.35 -6.35)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_L9.1mm_W9.1mm_Px6.35mm_Py6.35mm_Pulse_LP-25.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
