(footprint "L_SELF1408"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Self Ferrite 14 - 08")
	(tags "SELF")
	(property "Reference" "REF**"
		(at 7.72 -8.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_SELF1408"
		(at 7.82 9.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.62 2.54 0)
		(layer "F.Fab")
	)
	(pad "0" thru_hole circle
		(at 7.62 7.62)
		(size 2.03 2.03)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.03 2.03)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2.54 -2.54)
		(size 2.03 2.03)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 2.54 2.54)
		(size 2.03 2.03)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 12.7 -2.54)
		(size 2.03 2.03)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 12.7 2.54)
		(size 2.03 2.03)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 15.24 0)
		(size 2.03 2.03)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_SELF1408.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
