(footprint "L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
	(tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
	(property "Reference" "REF**"
		(at 0 -2.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm"
		(at 0 8.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.8 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 5.6)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
