(footprint "L_Wurth_WE-HCFT-2012_LeadDiameter1.2mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shielded High Current Inductor, body 17x22mm, https://www.we-online.com/catalog/en/WE-HCFT#/articles/WE-HCFT-2012-ROUND")
	(tags "THT")
	(property "Reference" "REF**"
		(at 6.5 -12.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "L_Wurth_WE-HCFT-2012_LeadDiameter1.2mm"
		(at 6.5 12.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 6.5 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 13 0)
		(size 2.4 2.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT_Wurth.3dshapes/L_Wurth_WE-HCFT-2012_LeadDiameter1.2mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
