(footprint "LED-L1T2_LUMILEDS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.lumileds.com/uploads/438/DS133-pdf")
	(tags "LUMILEDS LUXEON TX L1T2 LED")
	(property "Reference" "REF**"
		(at 0 2.58 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED-L1T2_LUMILEDS"
		(at 0 -3.42 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at 0.45 0.52)
		(size 0.55 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.45 0.52)
		(size 0.55 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -0.52)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED-L1T2_LUMILEDS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
