(footprint "LED_1206_3216Metric_ReverseMount_Hole1.8x2.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LED SMD 1206 (3216 Metric), reverse mount, square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
	(tags "diode reverse")
	(property "Reference" "REF**"
		(at 0 -2.145 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_1206_3216Metric_ReverseMount_Hole1.8x2.4mm"
		(at 0 2.145 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole oval
		(at 0 0)
		(size 1.8 2.4)
		(drill oval 1.8 2.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -1.55 0)
		(size 0.95 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "2" smd roundrect
		(at 1.55 0)
		(size 0.95 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric_ReverseMount.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
