(footprint "LED_CSP_Samsung_LH181B_2.36x2.36mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "High Power CSP LED, 2.36mm x 2.36mm, 1.4A max, https://cdn.samsung.com/led/file/resource/2021/01/Data_Sheet_LH181B_Rev.4.0.pdf")
	(tags "LED Samsung LH181B")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_CSP_Samsung_LH181B_2.36x2.36mm"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.39 0 90)
		(size 1.3 0.53)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.39 0 90)
		(size 1.3 0.53)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_CSP_Samsung_LH181B_2.36x2.36mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
