(footprint "LED_Cree-XHP70_6V"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Cree XHP70 LED, 6V version, http://www.cree.com/~/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP70.pdf")
	(tags "LED Cree XHP70")
	(property "Reference" "REF**"
		(at 0 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Cree-XHP70_6V"
		(at 0 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -3 -1.815)
		(size 0.7 3.13)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -3 1.815)
		(size 0.7 3.13)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.77 -2.31)
		(size 1.29 1.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.77 -0.77)
		(size 1.29 1.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.77 0.77)
		(size 1.29 1.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.77 2.31)
		(size 1.29 1.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.77 -2.31)
		(size 1.29 1.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.77 -0.77)
		(size 1.29 1.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.77 0.77)
		(size 1.29 1.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.77 2.31)
		(size 1.29 1.29)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3 -1.815)
		(size 0.7 3.13)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3 1.815)
		(size 0.7 3.13)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -3 0)
		(size 0.7 6.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 3 0)
		(size 0.7 6.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at 0 0)
		(size 3.9 6.76)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Cree-XHP70_6V.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
