(footprint "LED_Luminus_MP-3030-1100_3.0x3.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mid Power LED, Luminus MP-3030-1100, 3.0x3.0mm, 816mW, https://download.luminus.com/datasheets/Luminus_MP3030_1100_Datasheet.pdf")
	(tags "LED Luminus MP-3030-1100")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Luminus_MP-3030-1100_3.0x3.0mm"
		(at 0 2.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.575 0)
		(size 1.3 1.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.075 0)
		(size 0.4 1.9)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -0.575 0)
		(size 1.6 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 1.075 0)
		(size 0.6 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 1.375 0)
		(size 0.6 0.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Luminus_MP-3030-1100_3.0x3.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
