(footprint "LED_RGB_Getian_GT-P6PRGB4303"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.gme.sk/img/cache/doc/518/177/vykonova-led-getian-gt-p6prgb4303-datasheet-1.pdf")
	(tags "LED RGB ")
	(property "Reference" "REF**"
		(at 0 -5.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_RGB_Getian_GT-P6PRGB4303"
		(at 0 5.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -6.22 -1.7)
		(size 3.1 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.22 0)
		(size 3.1 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.22 1.7)
		(size 3.1 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 6.22 1.7 180)
		(size 3.1 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 6.22 0 180)
		(size 3.1 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 6.22 -1.7 180)
		(size 3.1 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "PAD" smd circle
		(at 0 0)
		(size 5.7 5.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_RGB_Getian_GT-P6PRGB4303.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
