(footprint "LED_Rectangular_W7.62mm_H4.55mm_P5.08mm_R3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Datasheet can be found at https://www.gme.cz/data/attachments/dsh.511-795.1.pdf")
	(tags "LED automotive super flux 7.62mm")
	(property "Reference" "REF**"
		(at 1.27 -2.54 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Rectangular_W7.62mm_H4.55mm_P5.08mm_R3"
		(at 3.81 7.62 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -2.286 -1.27 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.8 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 5.08 0)
		(size 1.8 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 5.08)
		(size 1.8 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 5.08)
		(size 1.8 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_Rectangular_W7.62mm_H4.55mm_P5.08mm_R3.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
