(footprint "MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mounting Hole 2.7mm, M2.5, DIN965")
	(tags "mounting hole 2.7mm m2.5 din965")
	(property "Reference" "REF**"
		(at 0 -3.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "MountingHole_2.7mm_M2.5_DIN965_Pad_TopOnly"
		(at 0 3.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3.1 3.1)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" connect circle
		(at 0 0)
		(size 4.7 4.7)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
