(footprint "MountingHole_4.3x6.2mm_M4_Pad_Via"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mounting Hole 4.3x6.2mm, M4")
	(tags "mounting hole 4.3x6.2mm m4")
	(property "Reference" "REF**"
		(at 0 -5.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "MountingHole_4.3x6.2mm_M4_Pad_Via"
		(at 0 5.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -4.15 0)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -3.801 -1.45)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -3.801 1.45)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.92 -2.521)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -2.92 2.521)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -1.505 -3.151)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at -1.505 3.151)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 0 -3.225)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 10.4 8.6)
		(drill oval 6.2 4.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 3.225)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 1.505 -3.151)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 1.505 3.151)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.92 -2.521)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 2.92 2.521)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 3.801 -1.45)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 3.801 1.45)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "1" thru_hole circle
		(at 4.15 0)
		(size 0.9 0.9)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(embedded_fonts no)
)
