(footprint "MountingHole_5.3mm_M5_ISO14580_Pad"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mounting Hole 5.3mm, M5, ISO14580")
	(tags "mounting hole 5.3mm m5 iso14580")
	(property "Reference" "REF**"
		(at 0 -5.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "MountingHole_5.3mm_M5_ISO14580_Pad"
		(at 0 5.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 8.5 8.5)
		(drill 5.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
