(footprint "MountingHole_5.3mm_M5_ISO7380_Pad_TopOnly"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mounting Hole 5.3mm, M5, ISO7380")
	(tags "mounting hole 5.3mm m5 iso7380")
	(property "Reference" "REF**"
		(at 0 -5.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "MountingHole_5.3mm_M5_ISO7380_Pad_TopOnly"
		(at 0 5.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 5.7 5.7)
		(drill 5.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" connect circle
		(at 0 0)
		(size 9.5 9.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
