(footprint "ToolingHole_1.152mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Tooling Hole 1.152mm, 1.3mm solder mask, JLCPCB specification, https://jlcpcb.com/help/article/How-to-add-tooling-holes-for-PCB-assembly-order")
	(tags "mounting")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "ToolingHole_1.152mm"
		(at 0 1.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 1.152 1.152)
		(drill 1.152)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 0.074)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0.7 0) (xy 0.679659 -0.167521) (xy 0.619819 -0.325306) (xy 0.523958 -0.464186) (xy 0.397645 -0.576089)
				(xy 0.248223 -0.654511) (xy 0.084376 -0.694896) (xy -0.084376 -0.694896) (xy -0.248223 -0.654511)
				(xy -0.397645 -0.576089) (xy -0.523958 -0.464186) (xy -0.619819 -0.325306) (xy -0.679659 -0.167521)
				(xy -0.7 0) (xy -0.679659 0.167521) (xy -0.619819 0.325306) (xy -0.523958 0.464186) (xy -0.397645 0.576089)
				(xy -0.248223 0.654511) (xy -0.084376 0.694896) (xy 0.084376 0.694896) (xy 0.248223 0.654511) (xy 0.397645 0.576089)
				(xy 0.523958 0.464186) (xy 0.619819 0.325306) (xy 0.679659 0.167521)
			)
		)
	)
	(embedded_fonts no)
)
