(footprint "Mounting_Wuerth_WA-SMSE-ExternalM3_H9mm_9771090360"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, external M3, height 9, Wuerth electronics 9771090360 (https://katalog.we-online.com/em/datasheet/9771090360.pdf), generated with kicad-footprint-generator")
	(tags "Mounting M3 9771090360")
	(property "Reference" "REF**"
		(at 0 -4.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMSE-ExternalM3_H9mm_9771090360"
		(at 0 4.65 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at 0 -2.1)
		(size 1.5 1.5)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.305123 1.47)
				(mid 0.371762 1.506879)
				(end 0.7 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.493052 1.47)
				(mid 0.350399 1.380819)
				(end 0.8 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.642729 1.47)
				(mid 0.340253 1.266797)
				(end 0.9 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.776595 1.47)
				(mid 0.334219 1.157505)
				(end 1 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -0.901721 1.47)
				(mid 0.330233 1.05074)
				(end 1.1 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.021323 1.47)
				(mid 0.327424 0.945533)
				(end 1.2 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.137146 1.47)
				(mid 0.325354 0.841372)
				(end 1.3 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.25024 1.47)
				(mid 0.323778 0.737954)
				(end 1.4 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.361286 1.47)
				(mid 0.322545 0.635089)
				(end 1.5 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.470748 1.47)
				(mid 0.321561 0.532646)
				(end 1.6 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.578955 1.47)
				(mid 0.320762 0.430535)
				(end 1.7 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.686149 1.47)
				(mid 0.320102 0.328691)
				(end 1.8 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.792512 1.47)
				(mid 0.319552 0.227065)
				(end 1.9 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -1.898183 1.47)
				(mid 0.319087 0.125618)
				(end 2 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.003272 1.47)
				(mid 0.318691 0.024323)
				(end 2.1 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.107866 1.47)
				(mid 0.318351 -0.076845)
				(end 2.2 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.212035 1.47)
				(mid 0.318056 -0.177903)
				(end 2.3 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.315837 1.47)
				(mid 0.317798 -0.278866)
				(end 2.4 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.419318 1.47)
				(mid 0.317573 -0.379747)
				(end 2.5 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.522519 1.47)
				(mid 0.317373 -0.480557)
				(end 2.6 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.625471 1.47)
				(mid 0.317197 -0.581303)
				(end 2.7 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.728205 1.47)
				(mid 0.317039 -0.681993)
				(end 2.8 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.830742 1.47)
				(mid 0.316898 -0.782633)
				(end 2.9 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -2.933104 1.47)
				(mid 0.316771 -0.883229)
				(end 3 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -3.035309 1.47)
				(mid 0.316656 -0.983785)
				(end 3.1 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -3.137372 1.47)
				(mid 0.316553 -1.084304)
				(end 3.2 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -3.239305 1.47)
				(mid 0.316458 -1.184791)
				(end 3.3 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -3.341123 1.47)
				(mid 0.316373 -1.285249)
				(end 3.4 2.1)
				(width 0.2)
			)
			(gr_arc
				(start -3.442833 1.47)
				(mid 0.316294 -1.385679)
				(end 3.5 2.1)
				(width 0.2)
			)
			(gr_line
				(start 0.7 2.1)
				(end 3.5 2.1)
				(width 0.2)
			)
			(gr_line
				(start -0.305123 1.47)
				(end -3.442833 1.47)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 0 2.1)
		(size 1.5 1.5)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.305123 -1.47)
				(mid -0.371762 -1.506879)
				(end -0.7 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 0.493052 -1.47)
				(mid -0.350399 -1.380819)
				(end -0.8 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 0.642729 -1.47)
				(mid -0.340253 -1.266797)
				(end -0.9 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 0.776595 -1.47)
				(mid -0.334219 -1.157505)
				(end -1 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 0.901721 -1.47)
				(mid -0.330233 -1.05074)
				(end -1.1 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.021323 -1.47)
				(mid -0.327424 -0.945533)
				(end -1.2 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.137146 -1.47)
				(mid -0.325354 -0.841372)
				(end -1.3 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.25024 -1.47)
				(mid -0.323778 -0.737954)
				(end -1.4 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.361286 -1.47)
				(mid -0.322545 -0.635089)
				(end -1.5 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.470748 -1.47)
				(mid -0.321561 -0.532646)
				(end -1.6 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.578955 -1.47)
				(mid -0.320762 -0.430535)
				(end -1.7 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.686149 -1.47)
				(mid -0.320102 -0.328691)
				(end -1.8 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.792512 -1.47)
				(mid -0.319552 -0.227065)
				(end -1.9 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 1.898183 -1.47)
				(mid -0.319087 -0.125618)
				(end -2 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.003272 -1.47)
				(mid -0.318691 -0.024323)
				(end -2.1 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.107866 -1.47)
				(mid -0.318351 0.076845)
				(end -2.2 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.212035 -1.47)
				(mid -0.318056 0.177903)
				(end -2.3 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.315837 -1.47)
				(mid -0.317798 0.278866)
				(end -2.4 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.419318 -1.47)
				(mid -0.317573 0.379747)
				(end -2.5 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.522519 -1.47)
				(mid -0.317373 0.480557)
				(end -2.6 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.625471 -1.47)
				(mid -0.317197 0.581303)
				(end -2.7 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.728205 -1.47)
				(mid -0.317039 0.681993)
				(end -2.8 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.830742 -1.47)
				(mid -0.316898 0.782633)
				(end -2.9 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 2.933104 -1.47)
				(mid -0.316771 0.883229)
				(end -3 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 3.035309 -1.47)
				(mid -0.316656 0.983785)
				(end -3.1 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 3.137372 -1.47)
				(mid -0.316553 1.084304)
				(end -3.2 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 3.239305 -1.47)
				(mid -0.316458 1.184791)
				(end -3.3 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 3.341123 -1.47)
				(mid -0.316373 1.285249)
				(end -3.4 -2.1)
				(width 0.2)
			)
			(gr_arc
				(start 3.442833 -1.47)
				(mid -0.316294 1.385679)
				(end -3.5 -2.1)
				(width 0.2)
			)
			(gr_line
				(start -0.7 -2.1)
				(end -3.5 -2.1)
				(width 0.2)
			)
			(gr_line
				(start 0.305123 -1.47)
				(end 3.442833 -1.47)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -2.1 0)
		(size 2.692 2.692)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -2.1)
		(size 2.692 2.692)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 2.1)
		(size 2.692 2.692)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 2.1 0)
		(size 3.2 3.2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -2.1 0)
				(end 0 0)
				(width 3.2)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMSE-ExternalM3_H9mm_9771090360.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
