(footprint "Mounting_Wuerth_WA-SMSI-4.5mm_H9mm_9774090482"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside through hole 4.5mm, height 9, Wuerth electronics 9774090482 (https://katalog.we-online.de/em/datasheet/9774090482.pdf), generated with kicad-footprint-generator")
	(tags "Mounting 4.5mm 9774090482")
	(property "Reference" "REF**"
		(at 0 -5.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMSI-4.5mm_H9mm_9774090482"
		(at 0 5.65 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -2.607456 -2.607456)
		(size 0.9475 0.9475)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.188183 2.107456)
				(mid 0.599273 0.599273)
				(end 2.107456 -0.188183)
				(width 0.2)
			)
			(gr_arc
				(start -0.289416 2.107456)
				(mid 0.52877 0.52877)
				(end 2.107456 -0.289416)
				(width 0.2)
			)
			(gr_arc
				(start -0.390547 2.107456)
				(mid 0.458268 0.458268)
				(end 2.107456 -0.390547)
				(width 0.2)
			)
			(gr_arc
				(start -0.491585 2.107456)
				(mid 0.387765 0.387765)
				(end 2.107456 -0.491585)
				(width 0.2)
			)
			(gr_arc
				(start -0.59254 2.107456)
				(mid 0.317262 0.317262)
				(end 2.107456 -0.59254)
				(width 0.2)
			)
			(gr_arc
				(start -0.693419 2.107456)
				(mid 0.246759 0.246759)
				(end 2.107456 -0.693419)
				(width 0.2)
			)
			(gr_arc
				(start -0.794229 2.107456)
				(mid 0.176257 0.176257)
				(end 2.107456 -0.794229)
				(width 0.2)
			)
			(gr_arc
				(start -0.894975 2.107456)
				(mid 0.105754 0.105754)
				(end 2.107456 -0.894975)
				(width 0.2)
			)
			(gr_arc
				(start -0.995664 2.107456)
				(mid 0.035251 0.035251)
				(end 2.107456 -0.995664)
				(width 0.2)
			)
			(gr_arc
				(start -1.0963 2.107456)
				(mid -0.035251 -0.035251)
				(end 2.107456 -1.0963)
				(width 0.2)
			)
			(gr_arc
				(start -1.196886 2.107456)
				(mid -0.105754 -0.105754)
				(end 2.107456 -1.196886)
				(width 0.2)
			)
			(gr_arc
				(start -1.297427 2.107456)
				(mid -0.176257 -0.176257)
				(end 2.107456 -1.297427)
				(width 0.2)
			)
			(gr_arc
				(start -1.397927 2.107456)
				(mid -0.246759 -0.246759)
				(end 2.107456 -1.397927)
				(width 0.2)
			)
			(gr_arc
				(start -1.498388 2.107456)
				(mid -0.317262 -0.317262)
				(end 2.107456 -1.498388)
				(width 0.2)
			)
			(gr_arc
				(start -1.598813 2.107456)
				(mid -0.387765 -0.387765)
				(end 2.107456 -1.598813)
				(width 0.2)
			)
			(gr_arc
				(start -1.699204 2.107456)
				(mid -0.458268 -0.458268)
				(end 2.107456 -1.699204)
				(width 0.2)
			)
			(gr_arc
				(start -1.799565 2.107456)
				(mid -0.52877 -0.52877)
				(end 2.107456 -1.799565)
				(width 0.2)
			)
			(gr_arc
				(start -1.899896 2.107456)
				(mid -0.599273 -0.599273)
				(end 2.107456 -1.899896)
				(width 0.2)
			)
			(gr_arc
				(start -1.899896 2.107456)
				(mid -0.599273 -0.599273)
				(end 2.107456 -1.899896)
				(width 0.2)
			)
			(gr_line
				(start 2.107456 -0.188183)
				(end 2.107456 -1.899896)
				(width 0.2)
			)
			(gr_line
				(start -0.188183 2.107456)
				(end -1.899896 2.107456)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -2.607456 2.607456)
		(size 0.9475 0.9475)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 2.107456 0.188183)
				(mid 0.599273 -0.599273)
				(end -0.188183 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 0.289416)
				(mid 0.52877 -0.52877)
				(end -0.289416 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 0.390547)
				(mid 0.458268 -0.458268)
				(end -0.390547 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 0.491585)
				(mid 0.387765 -0.387765)
				(end -0.491585 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 0.59254)
				(mid 0.317262 -0.317262)
				(end -0.59254 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 0.693419)
				(mid 0.246759 -0.246759)
				(end -0.693419 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 0.794229)
				(mid 0.176257 -0.176257)
				(end -0.794229 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 0.894975)
				(mid 0.105754 -0.105754)
				(end -0.894975 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 0.995664)
				(mid 0.035251 -0.035251)
				(end -0.995664 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.0963)
				(mid -0.035251 0.035251)
				(end -1.0963 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.196886)
				(mid -0.105754 0.105754)
				(end -1.196886 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.297427)
				(mid -0.176257 0.176257)
				(end -1.297427 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.397927)
				(mid -0.246759 0.246759)
				(end -1.397927 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.498388)
				(mid -0.317262 0.317262)
				(end -1.498388 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.598813)
				(mid -0.387765 0.387765)
				(end -1.598813 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.699204)
				(mid -0.458268 0.458268)
				(end -1.699204 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.799565)
				(mid -0.52877 0.52877)
				(end -1.799565 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.899896)
				(mid -0.599273 0.599273)
				(end -1.899896 -2.107456)
				(width 0.2)
			)
			(gr_arc
				(start 2.107456 1.899896)
				(mid -0.599273 0.599273)
				(end -1.899896 -2.107456)
				(width 0.2)
			)
			(gr_line
				(start -0.188183 -2.107456)
				(end -1.899896 -2.107456)
				(width 0.2)
			)
			(gr_line
				(start 2.107456 0.188183)
				(end 2.107456 1.899896)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 5.4 5.4)
		(drill 5.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 2.607456 -2.607456)
		(size 0.9475 0.9475)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -2.107456 -0.188183)
				(mid -0.599273 0.599273)
				(end 0.188183 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -0.289416)
				(mid -0.52877 0.52877)
				(end 0.289416 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -0.390547)
				(mid -0.458268 0.458268)
				(end 0.390547 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -0.491585)
				(mid -0.387765 0.387765)
				(end 0.491585 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -0.59254)
				(mid -0.317262 0.317262)
				(end 0.59254 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -0.693419)
				(mid -0.246759 0.246759)
				(end 0.693419 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -0.794229)
				(mid -0.176257 0.176257)
				(end 0.794229 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -0.894975)
				(mid -0.105754 0.105754)
				(end 0.894975 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -0.995664)
				(mid -0.035251 0.035251)
				(end 0.995664 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.0963)
				(mid 0.035251 -0.035251)
				(end 1.0963 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.196886)
				(mid 0.105754 -0.105754)
				(end 1.196886 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.297427)
				(mid 0.176257 -0.176257)
				(end 1.297427 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.397927)
				(mid 0.246759 -0.246759)
				(end 1.397927 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.498388)
				(mid 0.317262 -0.317262)
				(end 1.498388 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.598813)
				(mid 0.387765 -0.387765)
				(end 1.598813 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.699204)
				(mid 0.458268 -0.458268)
				(end 1.699204 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.799565)
				(mid 0.52877 -0.52877)
				(end 1.799565 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.899896)
				(mid 0.599273 -0.599273)
				(end 1.899896 2.107456)
				(width 0.2)
			)
			(gr_arc
				(start -2.107456 -1.899896)
				(mid 0.599273 -0.599273)
				(end 1.899896 2.107456)
				(width 0.2)
			)
			(gr_line
				(start 0.188183 2.107456)
				(end 1.899896 2.107456)
				(width 0.2)
			)
			(gr_line
				(start -2.107456 -0.188183)
				(end -2.107456 -1.899896)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.607456 2.607456)
		(size 0.9475 0.9475)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.188183 -2.107456)
				(mid -0.599273 -0.599273)
				(end -2.107456 0.188183)
				(width 0.2)
			)
			(gr_arc
				(start 0.289416 -2.107456)
				(mid -0.52877 -0.52877)
				(end -2.107456 0.289416)
				(width 0.2)
			)
			(gr_arc
				(start 0.390547 -2.107456)
				(mid -0.458268 -0.458268)
				(end -2.107456 0.390547)
				(width 0.2)
			)
			(gr_arc
				(start 0.491585 -2.107456)
				(mid -0.387765 -0.387765)
				(end -2.107456 0.491585)
				(width 0.2)
			)
			(gr_arc
				(start 0.59254 -2.107456)
				(mid -0.317262 -0.317262)
				(end -2.107456 0.59254)
				(width 0.2)
			)
			(gr_arc
				(start 0.693419 -2.107456)
				(mid -0.246759 -0.246759)
				(end -2.107456 0.693419)
				(width 0.2)
			)
			(gr_arc
				(start 0.794229 -2.107456)
				(mid -0.176257 -0.176257)
				(end -2.107456 0.794229)
				(width 0.2)
			)
			(gr_arc
				(start 0.894975 -2.107456)
				(mid -0.105754 -0.105754)
				(end -2.107456 0.894975)
				(width 0.2)
			)
			(gr_arc
				(start 0.995664 -2.107456)
				(mid -0.035251 -0.035251)
				(end -2.107456 0.995664)
				(width 0.2)
			)
			(gr_arc
				(start 1.0963 -2.107456)
				(mid 0.035251 0.035251)
				(end -2.107456 1.0963)
				(width 0.2)
			)
			(gr_arc
				(start 1.196886 -2.107456)
				(mid 0.105754 0.105754)
				(end -2.107456 1.196886)
				(width 0.2)
			)
			(gr_arc
				(start 1.297427 -2.107456)
				(mid 0.176257 0.176257)
				(end -2.107456 1.297427)
				(width 0.2)
			)
			(gr_arc
				(start 1.397927 -2.107456)
				(mid 0.246759 0.246759)
				(end -2.107456 1.397927)
				(width 0.2)
			)
			(gr_arc
				(start 1.498388 -2.107456)
				(mid 0.317262 0.317262)
				(end -2.107456 1.498388)
				(width 0.2)
			)
			(gr_arc
				(start 1.598813 -2.107456)
				(mid 0.387765 0.387765)
				(end -2.107456 1.598813)
				(width 0.2)
			)
			(gr_arc
				(start 1.699204 -2.107456)
				(mid 0.458268 0.458268)
				(end -2.107456 1.699204)
				(width 0.2)
			)
			(gr_arc
				(start 1.799565 -2.107456)
				(mid 0.52877 0.52877)
				(end -2.107456 1.799565)
				(width 0.2)
			)
			(gr_arc
				(start 1.899896 -2.107456)
				(mid 0.599273 0.599273)
				(end -2.107456 1.899896)
				(width 0.2)
			)
			(gr_arc
				(start 1.899896 -2.107456)
				(mid 0.599273 0.599273)
				(end -2.107456 1.899896)
				(width 0.2)
			)
			(gr_line
				(start -2.107456 0.188183)
				(end -2.107456 1.899896)
				(width 0.2)
			)
			(gr_line
				(start 0.188183 -2.107456)
				(end 1.899896 -2.107456)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -3.7 0)
		(size 1.492 1.492)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -3.7)
		(size 1.492 1.492)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 3.7)
		(size 1.492 1.492)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 3.7 0)
		(size 2 2)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -3.7 0)
				(end 0 0)
				(width 2)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMSI-4.5mm_H9mm_9774090482.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
