(footprint "Mounting_Wuerth_WA-SMST-3.3mm_H14mm_9774140960"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside through hole 3.3mm, height 14, Wuerth electronics 9774140960 (https://katalog.we-online.de/em/datasheet/9774140960.pdf,), generated with kicad-footprint-generator")
	(tags "Mounting 3.3mm 9774140960")
	(property "Reference" "REF**"
		(at 0 -4.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMST-3.3mm_H14mm_9774140960"
		(at 0 4.65 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -2.057681 -2.057681)
		(size 0.55 0.55)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.377294 1.707681)
				(mid 0.318198 0.318198)
				(end 1.707681 -0.377294)
				(width 0.2)
			)
			(gr_arc
				(start -0.478281 1.707681)
				(mid 0.247487 0.247487)
				(end 1.707681 -0.478281)
				(width 0.2)
			)
			(gr_arc
				(start -0.579192 1.707681)
				(mid 0.176777 0.176777)
				(end 1.707681 -0.579192)
				(width 0.2)
			)
			(gr_arc
				(start -0.680037 1.707681)
				(mid 0.106066 0.106066)
				(end 1.707681 -0.680037)
				(width 0.2)
			)
			(gr_arc
				(start -0.780822 1.707681)
				(mid 0.035355 0.035355)
				(end 1.707681 -0.780822)
				(width 0.2)
			)
			(gr_arc
				(start -0.881554 1.707681)
				(mid -0.035355 -0.035355)
				(end 1.707681 -0.881554)
				(width 0.2)
			)
			(gr_arc
				(start -0.982237 1.707681)
				(mid -0.106066 -0.106066)
				(end 1.707681 -0.982237)
				(width 0.2)
			)
			(gr_arc
				(start -1.082877 1.707681)
				(mid -0.176777 -0.176777)
				(end 1.707681 -1.082877)
				(width 0.2)
			)
			(gr_arc
				(start -1.183476 1.707681)
				(mid -0.247487 -0.247487)
				(end 1.707681 -1.183476)
				(width 0.2)
			)
			(gr_arc
				(start -1.28404 1.707681)
				(mid -0.318198 -0.318198)
				(end 1.707681 -1.28404)
				(width 0.2)
			)
			(gr_line
				(start 1.707681 -0.377294)
				(end 1.707681 -1.28404)
				(width 0.2)
			)
			(gr_line
				(start -0.377294 1.707681)
				(end -1.28404 1.707681)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -2.057681 2.057681)
		(size 0.55 0.55)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 1.707681 0.377294)
				(mid 0.318198 -0.318198)
				(end -0.377294 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.478281)
				(mid 0.247487 -0.247487)
				(end -0.478281 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.579192)
				(mid 0.176777 -0.176777)
				(end -0.579192 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.680037)
				(mid 0.106066 -0.106066)
				(end -0.680037 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.780822)
				(mid 0.035355 -0.035355)
				(end -0.780822 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.881554)
				(mid -0.035355 0.035355)
				(end -0.881554 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.982237)
				(mid -0.106066 0.106066)
				(end -0.982237 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 1.082877)
				(mid -0.176777 0.176777)
				(end -1.082877 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 1.183476)
				(mid -0.247487 0.247487)
				(end -1.183476 -1.707681)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 1.28404)
				(mid -0.318198 0.318198)
				(end -1.28404 -1.707681)
				(width 0.2)
			)
			(gr_line
				(start -0.377294 -1.707681)
				(end -1.28404 -1.707681)
				(width 0.2)
			)
			(gr_line
				(start 1.707681 0.377294)
				(end 1.707681 1.28404)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 4.4 4.4)
		(drill 4.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 2.057681 -2.057681)
		(size 0.55 0.55)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -1.707681 -0.377294)
				(mid -0.318198 0.318198)
				(end 0.377294 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.478281)
				(mid -0.247487 0.247487)
				(end 0.478281 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.579192)
				(mid -0.176777 0.176777)
				(end 0.579192 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.680037)
				(mid -0.106066 0.106066)
				(end 0.680037 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.780822)
				(mid -0.035355 0.035355)
				(end 0.780822 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.881554)
				(mid 0.035355 -0.035355)
				(end 0.881554 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.982237)
				(mid 0.106066 -0.106066)
				(end 0.982237 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -1.082877)
				(mid 0.176777 -0.176777)
				(end 1.082877 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -1.183476)
				(mid 0.247487 -0.247487)
				(end 1.183476 1.707681)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -1.28404)
				(mid 0.318198 -0.318198)
				(end 1.28404 1.707681)
				(width 0.2)
			)
			(gr_line
				(start 0.377294 1.707681)
				(end 1.28404 1.707681)
				(width 0.2)
			)
			(gr_line
				(start -1.707681 -0.377294)
				(end -1.707681 -1.28404)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.057681 2.057681)
		(size 0.55 0.55)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.377294 -1.707681)
				(mid -0.318198 -0.318198)
				(end -1.707681 0.377294)
				(width 0.2)
			)
			(gr_arc
				(start 0.478281 -1.707681)
				(mid -0.247487 -0.247487)
				(end -1.707681 0.478281)
				(width 0.2)
			)
			(gr_arc
				(start 0.579192 -1.707681)
				(mid -0.176777 -0.176777)
				(end -1.707681 0.579192)
				(width 0.2)
			)
			(gr_arc
				(start 0.680037 -1.707681)
				(mid -0.106066 -0.106066)
				(end -1.707681 0.680037)
				(width 0.2)
			)
			(gr_arc
				(start 0.780822 -1.707681)
				(mid -0.035355 -0.035355)
				(end -1.707681 0.780822)
				(width 0.2)
			)
			(gr_arc
				(start 0.881554 -1.707681)
				(mid 0.035355 0.035355)
				(end -1.707681 0.881554)
				(width 0.2)
			)
			(gr_arc
				(start 0.982237 -1.707681)
				(mid 0.106066 0.106066)
				(end -1.707681 0.982237)
				(width 0.2)
			)
			(gr_arc
				(start 1.082877 -1.707681)
				(mid 0.176777 0.176777)
				(end -1.707681 1.082877)
				(width 0.2)
			)
			(gr_arc
				(start 1.183476 -1.707681)
				(mid 0.247487 0.247487)
				(end -1.707681 1.183476)
				(width 0.2)
			)
			(gr_arc
				(start 1.28404 -1.707681)
				(mid 0.318198 0.318198)
				(end -1.707681 1.28404)
				(width 0.2)
			)
			(gr_line
				(start -1.707681 0.377294)
				(end -1.707681 1.28404)
				(width 0.2)
			)
			(gr_line
				(start 0.377294 -1.707681)
				(end 1.28404 -1.707681)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -2.95 0)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -2.95)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 2.95)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 2.95 0)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -2.95 0)
				(end 0 0)
				(width 1.5)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMST-3.3mm_H14mm_9774140960.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
